######

###### KURO

###### Information for invitation to tender

**Product:**

#### PC/ABS Forwarding tube – halogenfree

* manufactured according to DIN 6660
* rated non-toxic with regard to the acute

inhalation toxicity

* fire classification **B-s1-d0**

(according to DIN EN 13501-1:2010-01)

**Text for Invitation to tender:**

|  |  |
| --- | --- |
| Pos: ....................... | PC/ABS Forwarding tube 108 x 4.0 x 5000 mm – **NW 100** |
|  | colour: light grey (according to RAL 7035) |
|  | material: PC/ABS Blend – halogenfree\* manufactured according to DIN 6660\* rated non-toxic with regard to the acute  inhalation toxicity\* fire classification **B-s1-d0** (according to DIN EN 13501-1:2010-01)\* connection with band hose clamps |
|  | System KURO or equal (www.kuro-kunststoffe.com)Quantity: ............ m Price/Unit: .......... Price total: .......... |

|  |  |
| --- | --- |
| Pos: ....................... | PC/ABS Forwarding tube 110 x 2.3 x 5000 mm – **NW 110** |
|  | colour: light grey (according to RAL 7035) |
|  | material: PC/ABS Blend – halogenfree\* manufactured according to DIN 6660\* rated non-toxic with regard to the acute  inhalation toxicity\* fire classification **B-s1-d0** (according to DIN EN 13501-1:2010-01)\* connection with wide band hose clamps |
|  | System KURO or equal (www.kuro-kunststoffe.com)Quantity: ............ m Price/Unit: .......... Price total: .......... |

|  |  |
| --- | --- |
| Pos: ....................... | PC/ABS Forwarding tube 160 x 3.2 x 5000 mm – **NW 160** |
|  | colour: light grey (according to RAL 7035) |
|  | material: PC/ABS Blend – halogenfree\* manufactured according to DIN 6660\* rated non-toxic with regard to the acute  inhalation toxicity\* fire classification **B-s1-d0** (according to DIN EN 13501-1:2010-01)\* connection with wide band hose clampsSystem KURO or equal (www.kuro-kunststoffe.com) |
|  | Quantity: ............ m Price/Unit: .......... Price total: .......... |