######  KURO

######  Information for invitation to tender



**Product:**

#### PEHD Underground bend

* Material: PE 100
* Operation temperature: -40°C up to +70°C

# Special dimension for pneumatic tube systems

**Text for Invitation to tender:**

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | PEHD Underground bend (pneumatic tube system) – **NW 90** |
|  |  | 110 x 12.0 mm, R = 1000 mm, 15° |
|  |  | 100 mm straight at both ends |
|  |  | colour: royal blue / PE 100 |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble |
|  |  |  |
|  |  | Quantity: ............ piece Price/Unit: .......... Price total: .......... |
|  |  |  |
|  | Pos: ....................... | PEHD Underground bend (pneumatic tube system) **– NW 90** |
|  |  | 110 x 12.0 mm, R = 1000 mm, 30° |
|  |  | 100 mm straight at both ends |
|  |  | colour: royal blue / PE 100 |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble |
|  |  |  |
|  |  | Quantity: ............ piece Price/Unit: .......... Price total: .......... |

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | PEHD Underground bend (pneumatic tube system) **– NW 90** |
|  |  | 110 x 12.0 mm, R = 1000 mm, 45° |
|  |  | 100 mm straight at both ends |
|  |  | colour: royal blue / PE 100 |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble |
|  |  |  |
|  |  | Quantity: ............ piece Price/Unit: .......... Price total: .......... |
|  |  |  |
|  | Pos: ....................... | PEHD Underground bend (pneumatic tube system) – **NW 90** |
|  |  | 110 x 12.0 mm, R = 1000 mm, 90° |
|  |  | 100 mm straight at both ends |
|  |  | colour: royal blue / PE 100 |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble |
|  |  |  |
|  |  | Quantity: ............ piece Price/Unit: .......... Price total: .......... |
|  | Pos: ....................... | PEHD Underground bend (pneumatic tube system**) – NW 100** |
|  |  | 125 x 12.5 mm, R = 1000 mm, 15° |
|  |  | 100 mm straight at both ends |
|  |  | colour: royal blue / PE 100 |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble |
|  |  |  |
|  |  | Quantity: ............ piece Price/Unit: .......... Price total: .......... |
|  |  |  |
|  | Pos: ....................... | PEHD Underground bend (pneumatic tube system) **– NW 100** |
|  |  | 125 x 12.5 mm, R = 1000 mm, 30° |
|  |  | 100 mm straight at both ends |
|  |  | colour: royal blue / PE 100 |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble |
|  |  |  |
|  |  | Quantity: ............ piece Price/Unit: .......... Price total: .......... |

|  |  |
| --- | --- |
|  Pos: ....................... | PEHD Underground bend (pneumatic tube system) **– NW 100** |
|  | 125 x 12.5 mm, R = 1000 mm, 45° |
|  | 100 mm straight at both ends |
|  | colour: royal blue / PE 100 |
|  | \* manufactured according to DIN 6660 |
|  | \* connection only with electrofusion coupler |
|  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  | System KURO or equal (www.kuro-kunststoffe.com) |
|  | deliver and assemble |
|  |  |
|  | Quantity: ............ piece Price/Unit: .......... Price total: .......... |
|  |  |
|  Pos: ....................... | PEHD Underground bend (pneumatic tube system) – **NW 100** |
|  | 125 x 12.5 mm, R = 1000 mm, 90° |
|  | 100 mm straight at both ends |
|  | colour: royal blue / PE 100 |
|  | \* manufactured according to DIN 6660 |
|  | \* connection only with electrofusion coupler |
|  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  | System KURO or equal (www.kuro-kunststoffe.com) |
|  | deliver and assemble |
|  |  |
|  | Quantity: ............ piece Price/Unit: .......... Price total: .......... |

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | PEHD Underground bend (pneumatic tube system) – **NW 110** |
|  |  | 125 x 9.8 mm, R = 1000 mm, 15° |
|  |  | 100 mm straight at both ends |
|  |  | colour: royal blue / PE 100 |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble |
|  |  |  |
|  |  | Quantity: ............ piece Price/Unit: .......... Price total: .......... |

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | PEHD Underground bend (pneumatic tube system) – **NW 110** |
|  |  | 125 x 9.8 mm, R = 1000 mm, 30° |
|  |  | 100 mm straight at both ends |
|  |  | colour: royal blue / PE 100 |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble |
|  |  |  |
|  |  | Quantity: ............ piece Price/Unit: .......... Price total: .......... |

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | PEHD Underground bend (pneumatic tube system) – **NW 110** |
|  |  | 125 x 9.8 mm, R = 1000 mm, 45° |
|  |  | 100 mm straight at both ends |
|  |  | colour: royal blue / PE 100 |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble |
|  |  |  |
|  |  | Quantity: ............ piece Price/Unit: .......... Price total: .......... |

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | PEHD Underground bend (pneumatic tube system) – **NW 110** |
|  |  | 125 x 9.8 mm, R = 1000 mm, 90° |
|  |  | 100 mm straight at both ends |
|  |  | colour: royal blue / PE 100 |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble |
|  |  |  |
|  |  | Quantity: ............ piece Price/Unit: .......... Price total: .......... |

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | PEHD Underground bend (pneumatic tube system) – **NW 160** |
|  |  | 200 x 23.2 mm, R = 1200 mm, 15° |
|  |  | 150 mm straight at both ends |
|  |  | colour: royal blue / PE 100 |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble |
|  |  |  |
|  |  | Quantity: ............ piece Price/Unit: .......... Price total: .......... |

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | PEHD Underground bend (pneumatic tube system) – **NW 160** |
|  |  | 200 x 23.2 mm, R = 1200 mm, 30° |
|  |  | 150 mm straight at both ends |
|  |  | colour: royal blue / PE 100 |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble |
|  |  |  |
|  |  | Quantity: ............ piece Price/Unit: .......... Price total: .......... |

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | PEHD Underground bend (pneumatic tube system) – **NW 160** |
|  |  | 200 x 23.2 mm, R = 1200 mm, 45° |
|  |  | 150 mm straight at both ends |
|  |  | colour: royal blue / PE 100 |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble |
|  |  |  |
|  |  | Quantity: ............ piece Price/Unit: .......... Price total: .......... |

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | PEHD Underground bend (pneumatic tube system) – **NW 160** |
|  |  | 200 x 23.2 mm, R = 1200 mm, 90° |
|  |  | 150 mm straight at both ends |
|  |  | colour: royal blue / PE 100 |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble |
|  |  |  |
|  |  | Quantity: ............ piece Price/Unit: .......... Price total: .......... |