######  KURO

######  Information for invitation to tender



**Product:**

#### PEHD Underground – covered

* Material: PE 100
* with composite insulation, foamed
* can be equipped with heating band
* Special dimension for pneumatic tube

**Text for Invitation to tender:**

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | PEHD Underground Bend (pneumatic tube system) **NW 90**  |
|  |  | with protective corrugated cover, foamed |
|  |  | Forwarding bend PEHD 110 x 12.0 mm, R = 1000 mm, 15°100 mm straight end at both ends, royal blue |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | Outer tube PEHD corrugated tube 175 x 20 mm, black |
|  |  | space between is filled with PU-foam |
|  |  | \* consider PEHD assembly instruction for Lamoltan foaming  |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble. |
|  |  |  |
|  |  | Quantity: ............ pc Price/Unit: .......... Price total: .......... |

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | PEHD Underground bend (pneumatic tube system) **NW 90**  |
|  |  | with protective corrugated cover, foamed |
|  |  | Forwarding bend PEHD 110 x 12.0 mm, R = 1000 mm, 30°100 mm straight end at both ends, royal blue |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | Outer tube PEHD corrugated pipe 175 x 20 mm, black |
|  |  | space between is filled with PU-foam |
|  |  | \* consider PEHD assembly instruction for Lamoltan foaming  |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble. |
|  |  |  |
|  |  | Quantity: ............ pc Price/Unit: .......... Price total: .......... |

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | PEHD Underground bend (pneumatic tube system) **NW 90**  |
|  |  | with protective corrugated cover, foamed |
|  |  | Forwarding bend PEHD 110 x 12.0 mm, R = 1000 mm, 45°100 mm straight end at both ends, royal blue |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider PEHD INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | Outer tube PEHD corrugated pipe 175 x 20 mm, black |
|  |  | space between is filled with PU-foam |
|  |  | \* consider PEHD assembly instruction for Lamoltan foaming  |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble. |
|  |  |  |
|  |  | Quantity: ............ pc Price/Unit: .......... Price total: .......... |

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | PEHD Underground bend (pneumatic tube system) **NW 90**  |
|  |  | with protective corrugated cover, foamed |
|  |  | Forwarding bend PEHD 110 x 12.0 mm, R = 1000 mm, 90°100 mm straight end at both ends, royal blue |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider PEHD INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | Outer tube PEHD corrugated pipe 175 x 20 mm, black |
|  |  | space between is filled with PU-foam |
|  |  | \* consider PEHD assembly instruction for Lamoltan foaming  |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble. |
|  |  |  |
|  |  | Quantity: ............ pc Price/Unit: .......... Price total: .......... |

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | PEHD Underground bend (pneumatic tube system) **NW 100** |
|  |  | with protective corrugated cover, foamed |
|  |  | Forwarding bend PEHD 125 x 12.5 mm, R = 1000 mm, 15°100 mm straight end at both ends, royal blue |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider PEHD INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | Outer tube PEHD corrugated pipe 135 x 20 mm, black |
|  |  | space between is filled with PU-foam |
|  |  | \* consider PEHD assembly instruction for Lamoltan foaming  |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble. |
|  |  |  |
|  |  | Quantity: ............ pc Price/Unit: .......... Price total: .......... |

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | PEHD Underground bend (pneumatic tube system) **NW 100** |
|  |  | with protective corrugated cover, foamed |
|  |  | Forwarding bend PEHD 125 x 12.5 mm, R = 1000 mm, 30°100 mm straight end at both ends, royal blue |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider PEHD INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | Outer tube PEHD corrugated pipe 135 x 20 mm, black |
|  |  | space between is filled with PU-foam |
|  |  | \* consider PEHD assembly instruction for Lamoltan foaming  |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble.Quantity: ............ pc Price/Unit: .......... Price total: .......... |
|  |  |  |
|  | Pos: ....................... | PEHD Underground bend (pneumatic tube system) **NW 100** |
|  |  | with protective corrugated cover, foamed |
|  |  | Forwarding bend PEHD 125 x 12.5 mm, R= 1000 mm, 45°100 mm straight end at both ends, royal blue |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | Outer tube PEHD corrugated pipe 135 x 20 mm, black |
|  |  | space between is filled with PU-foam |
|  |  | \* consider PEHD assembly instruction for Lamoltan foaming  |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble. |
|  |  |  |

 Quantity: ............ pc Price/Unit: .......... Price total: ..........

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | PEHD Underground Bend (pneumatic tube system) **NW 100** |
|  |  | with protective corrugated cover, foamed |
|  |  | Forwarding Bend PEHD 125 x 12.5 mm, R= 1000 mm, 90°100 mm straight end at both ends, royal blue |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | Outer tube PEHD corrugated pipe 135 x 20 mm, black |
|  |  | space between is filled with PU-foam |
|  |  | \* consider PEHD assembly instruction for Lamoltan foaming  |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble. |
|  |  |  |

 Quantity: ............ pc Price/Unit: .......... Price total: ..........

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | PEHD Underground bend (pneumatic tube system) **NW 110** |
|  |  | with protective corrugated cover, foamed |
|  |  | Forwarding bend PEHD 125 x 9.8 mm, R= 1000 mm, 15°100 mm straight end at both ends, royal blue |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | Outer tube PEHD corrugated pipe 135 x 20 mm, black |
|  |  | space between is filled with PU-foam |
|  |  | \* consider PEHD assembly instruction for Lamoltan foaming  |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble. |
|  |  |  |

 Quantity: ............ pc Price/Unit: .......... Price total: ..........

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | PEHD Underground bend (pneumatic tube system) **NW 110** |
|  |  | with protective corrugated cover, foamed |
|  |  | Forwarding bend PEHD 125 x 9.8 mm, R = 1000 mm, 30°100 mm straight end at both ends, royal blue |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | Outer tube PEHD corrugated pipe 135 x 20 mm, black |
|  |  | space between is filled with PU-foam |
|  |  | \* consider PEHD assembly instruction for Lamoltan foaming  |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble. |
|  |  |  |

 Quantity: ............ pc Price/Unit: .......... Price total: ..........

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | PEHD Underground bend (pneumatic tube system) **NW 110** |
|  |  | with protective corrugated cover, foamed |
|  |  | Forwarding bend PEHD 125 x 9.8 mm, R = 1000 mm, 45°100 mm straight end at both ends, royal blue |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | Outer tube PEHD corrugated pipe 135 x 20 mm, black |
|  |  | space between is filled with PU-foam |
|  |  | \* consider PEHD assembly instruction for Lamoltan foaming  |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble. |
|  |  |  |

 Quantity: ............ pc Price/Unit: .......... Price total: .......... |

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | PEHD Underground bend (pneumatic tube system) **NW 110** |
|  |  | with protective corrugated cover, foamed |
|  |  | Forwarding bend PEHD 125 x 9.8 mm, R = 1000 mm, 90°100 mm straight end at both ends, royal blue |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | Outer tube PEHD corrugated pipe 135 x 20 mm, black |
|  |  | space between is filled with PU-foam |
|  |  | \* consider PEHD assembly instruction for Lamoltan foaming  |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble. |
|  |  |  |

 Quantity: ............ pc Price/Unit: .......... Price total: ..........

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | PEHD Underground bend (pneumatic tube system) **NW 160** |
|  |  | with protective corrugated cover, foamed |
|  |  | Forwarding bend PEHD 200 x 23.2 mm, R = 1200 mm, 15°150 mm straight end at both ends, royal blue |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | Outer tube PEHD corrugated pipe 295 x 20 x 4700 mm, black |
|  |  | space between is filled with PU-foam |
|  |  | \* consider PEHD assembly instruction for Lamoltan foaming  |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble. |
|  |  |  |
|  |  | Quantity: ............ pc Price/Unit: .......... Price total: .......... |

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | PEHD Underground bend (pneumatic tube system) **NW 160** |
|  |  | with protective corrugated cover, foamed |
|  |  | Forwarding bend PEHD 200 x 23.2 mm, r = 1200 mm, 30°150 mm straight end at both ends, royal blue |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | Outer tube PEHD corrugated pipe 295 x 20 x 4700 mm, black |
|  |  | space between is filled with PU-foam |
|  |  | \* consider PEHD assembly instruction for Lamoltan foaming  |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble. |
|  |  |  |
|  |  | Quantity: ............ pc Price/Unit: .......... Price total: .......... |

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | PEHD Underground bend (pneumatic tube system) **NW 160** |
|  |  | with protective corrugated cover, foamed |
|  |  | Forwarding bend PEHD 200 x 23.2 mm, R= 1200 mm, 45°150 mm straight end at both ends, royal blue |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | Outer tube PEHD corrugated pipe 295 x 20 x 4700 mm, black |
|  |  | space between is filled with PU-foam |
|  |  | \* consider PEHD assembly instruction for Lamoltan foaming  |
|  |  | System KURO or equal (www.kuro-kunststoffe.com)deliver and assemble. |
|  |  |  |
|  |  | Quantity: ............ pc Price/Unit: .......... Price total: .......... |

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | PEHD Underground bend (pneumatic tube system) **NW 160** |
|  |  | with protective corrugated cover, foamed |
|  |  | Forwarding Bend PEHD 200 x 23.2 mm, R = 1200 mm, 90° 150 mm straight end at both ends, royal blue |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | Outer tube PEHD corrugated pipe 295 x 20 x 4700 mm, black |
|  |  | space between is filled with PU-foam |
|  |  | \* consider PEHD assembly instruction for Lamoltan foaming  |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble. |
|  |  |  |
|  |  | Quantity: ............ pc Price/Unit: .......... Price total: .......... |