
###### KURO

###### Information for invitation to tender

****

**Product:**

#### PEHD Underground tube - Covered

* Material: PE 100
* with composite insulation, foamed
* can be equipped with a heating band

# special dimension for pneumatic tube system

**Text for Invitation to tender:**

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | PEHD Underground tube (pneumatic tube system) **– NW 90** |
|  |  | with protective corrugated cover, foamed |
|  |  | Forwarding tube PEHD 110 x 12.0 mm, L = 5000 mm, royal blue |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | Outer tube PEHD corrugated pipe 174 x 10 x 4700 mm, black |
|  |  | space between is filled with PU-foam |
|  |  | \* consider PEHD assembly instruction for Lamalton foaming |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble. |
|  |  |  |
|  |  | Quantity: ............ m Price/Unit: .......... Price total: .......... |

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | PEHD Underground tube (pneumatic tube system) **– NW 100** |
|  |  | with protective corrugated cover, foamed |
|  |  | Forwarding tube PEHD 110 x 12.5 mm, L = 5000 mm, royal blue |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | Outer tube PEHD corrugated pipe 236 x 17 x 4700 mm, black |
|  |  | space between is filled with PU-foam |
|  |  | \* consider PEHD assembly instruction for Lamalton foaming |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble. |
|  |  |  |
|  |  | Quantity: ............ m Price/Unit: .......... Price total: .......... |
|  | Pos: ....................... | PEHD Underground tube (pneumatic tube system) – **NW 110** |
|  |  | with protective corrugated cover, foamed |
|  |  | Forwarding tube PEHD 125 x 9.8 mm, L = 5000 mm, royal blue |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | Outer tube PEHD corrugated pipe 236 x 17 x 4700 mm, black |
|  |  | space between is filled with PU-foam |
|  |  | \* consider PEHD assembly instruction for Lamalton foaming |
|  |  | System KURO or equal (www.kuro-kunststoffe.com) |
|  |  | deliver and assemble. |
|  |  |  |
|  |  | Quantity: ............ m Price/Unit: .......... Price total: .......... |

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | PEHD Underground tube (pneumatic tube system) **– NW 160** |
|  |  | with protective corrugated cover, foamed |
|  |  | Forwarding tube PEHD 200 x 23.2 mm, L = 5000 mm, royal blue |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider INSTRUCTION SHEET PEHD-UNDERGROUND TUBE SYSTEM |
|  |  | Outer tube PEHD corrugated pipe 290 x 20 x 4700 mm, black |
|  |  | space between is filled with PU-foam |
|  |  | \* consider PEHD assembly instruction for Lamalton foaming |
|  |  | System KURO or equal (www. www.kuro-kunststoffe.com) |
|  |  | deliver and assemble. |
|  |  |  |
|  |  | Quantity: ............ m Price/Unit: .......... Price total: .......... |