######  KURO

######  Information for invitation to tender

**Product:**

#### PEHD Underground Programme

#### \* with protective corrugated cover, foamed -

#### Underground Tube

Material: PE 100

# Special dimension for pneumatic tube system

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | **PEHD Underground Tube NW 90 (pneumatic tube system)** |
|  |  | **with protective corrugated cover, foamed** |
|  |  | Forwarding tube PEHD 110 x 12.0 mm, Length = 5000 mm, royal blue |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider PEHD pneumatic tube system assembly instruction |
|  |  | Outer tube PEHD corrugated pipe 174 x 10 x 4700 mm, black |
|  |  | space between is filled with PU-foam |
|  |  | \* consider PVC PTS instruction sheet  |
|  |  | System KURO or equal (www.kuro-kunststoffe.com),  |
|  |  | deliver and assemble. |
|  |  |  |
|  |  | Quantity: ............ m Price/Unit: .......... Price total: .......... |

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | **PEHD Underground Tube NW 100 (pneumatic tube system)** |
|  |  | **with protective corrugated cover, foamed** |
|  |  | Forwarding tube PEHD 125 x 12.5 mm, Length = 5000 mm, royal blue |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider PEHD pneumatic tube system assembly instruction |
|  |  | Outer tube PEHD corrugated pipe 236 x 17 x 4700 mm, black |
|  |  | space between is filled with PU-foam |
|  |  | \* consider PVC PTS instruction sheet  |
|  |  | System KURO or equal (www.kuro-kunststoffe.com),  |
|  |  | deliver and assemble. |
|  |  |  |
|  |  | Quantity: ............ m Price/Unit: .......... Price total: .......... |

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | **PEHD Underground Tube NW 110 (pneumatic tube system)** |
|  |  | **with protective corrugated cover, foamed** |
|  |  | Forwarding tube PEHD 125 x 9.8 mm, Length = 5000 mm, royal blue |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider PEHD pneumatic tube system assembly instruction |
|  |  | Outer tube PEHD corrugated pipe 236 x 17 x 4700 mm, black |
|  |  | space between is filled with PU-foam |
|  |  | \* consider PVC PTS instruction sheet  |
|  |  | System KURO or equal (www.kuro-kunststoffe.com),  |
|  |  | deliver and assemble. |
|  |  |  |
|  |  | Quantity: ............ m Price/Unit: .......... Price total: .......... |

|  |  |  |
| --- | --- | --- |
|  | Pos: ....................... | **PEHD Underground Tube NW 160 (pneumatic tube system)** |
|  |  | **with protective corrugated cover, foamed** |
|  |  | Forwarding tube PEHD 200 x 23.2 mm, Length = 5000 mm, royal blue |
|  |  | \* manufactured according to DIN 6660 |
|  |  | \* connection only with electrofusion coupler |
|  |  | \* consider PEHD pneumatic tube system assembly instruction |
|  |  | Outer tube PEHD corrugated pipe 295 x 20 x 4700 mm, black |
|  |  | space between is filled with PU-foam |
|  |  | \* consider PVC PTS instruction sheet  |
|  |  | System KURO or equal (www.kuro-kunststoffe.com),  |
|  |  | deliver and assemble. |
|  |  |  |
|  |  | Quantity: ............ m Price/Unit: .......... Price total: .......... |