######

###### KURO

###### Information for invitation to tender

**Product:**

#### PVC-U Forwarding tube - antibacterial CLEAN TUBE

* manufactured according to DIN 6660
* integrated antibacterial effect
* certified according to ASTM E 2180
* guaranteed antibacterial effect for up to 20 years

**Text for Invitation to tender:**

|  |  |
| --- | --- |
| Pos: ....................... | PVC-U Forwarding tube - antibacterial CLEAN TUBE **NW 110**110 x 2.3 mm, L= 5000 mm  |
|  | colour: iron grey (according to RAL 7011) or  silver grey (according to RAL 7001) |
|  | material: PVC-U / Microsilver\* manufactured according to DIN 6660\* certified according to ASTM E 2180\* guaranteed antibacterial effect for up to 20 years\* connection with PVC-collars or wide band hose clamps |
|  | System KURO or equal (www.kuro-kunststoffe.com)Quantity: ............ m Price/Unit: .......... Price total: .......... |

|  |  |
| --- | --- |
| Pos: ....................... | PVC-U Forwarding tube – antibacterial CLEAN TUBE **NW 160**160 x 3.2 mm, L= 5000 mm  |
|  | colour: iron grey (according to RAL 7011) or  silver grey (according to RAL 7001) |
|  | material: PVC-U / Microsilver\* manufactured according to DIN 6660\* certified according to ASTM E 2180\* guaranteed antibacterial effect for up to 20 years\* connection with PVC-collars or wide band hose clamps |
|  | System KURO or equal (www.kuro-kunststoffe.com)Quantity: ............ m Price/Unit: .......... Price total: .......... |